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GENERAL FEATURES

• MIDDLE RESOLUTION

• REQUIRES LOW LUX FOR LOW LIGHT APPLICATIONS

• AUTO ELECTRONIC SHUTTER

• BACK LIGHT COMPENSATION (BLC)

SPECIFICATIONS 

	Item No.
	CB-804B
	CC-9604B

	Description
	1/3” B/W Smoke Detector Camera
	1/4” Color DSP Smoke Detector Camera

	Pick up Element
	Sharp CCD Sensor
	Panasonic CCD Image Sensor

	Number of Pixels
	＜EIAC＞510(H)×492(V)

＜CCIR＞512(H)×582(V)
	＜NTSC＞510(H)×492(V)

＜PAL＞512(H)×582(V)

	Auto Electronics Shutter
	ON

	AGC
	ON

	BLC
	--
	ON

	Sync. Mode
	Internal Sync.

	Scanning System
	2:1 Interlace

	Resolution
	420 TV Lines

	S/N Ratio
	More than 48 dB

	Gamma Characteristic
	0.45

	Minimum illumination
	0.2 LUX, F/1.4
	0.92 LUX, F/1.4

	Horizontal Sync. Frequency
	＜EIA＞15.734 KHz

＜CCIR＞15.625KHz
	＜NTSC＞15.734 KHz

＜PAL＞15.625KHz

	Vertical Sync. Frequency
	60Hz(50Hz)

	Video Output
	1.0Vp-p, 75 ohm

	Power Source
	DC12V

	Power Consumption
	3.6W

	Operating Temperature
	-10℃ To +60℃

	Lens Amount
	f3.6mm Board Lens / F2.0

	Shutter Control
	＜EIA＞1/60-1/100,000 sec.

＜CCIR＞1/50-1/100,000 sec.
	＜NTSC＞1/60-1/100,000 sec.

＜PAL＞1/50-1/100,000 sec.

	Dimension
	130(Ø)×58(D)mm

	Net Weight
	0.35kg

	Exd. Model
	CB-804BA / with Audio
	CC-9604BA / with Audio
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